Building A needs addresses for 55 hosts:To accommodate 55 hosts, we need to find a subnet with at least 55 usable host addresses.To accommodate 55 hosts, we need a subnet with at least 64 (2^6) addresses, as it is the next available subnet size that can accommodate 55 hosts.
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