Initial water level: Initial water level of Karot break model is considered as NPL 461 m, initial water level between Karot damsite and Mangla damsite is considered as NPL 378.56 m of Mangla hydropower station; for the river reach with bed elevation higher than 378.56 m, its initial water level is considered according to the initial water level of adjacent river sections and the slope of river.
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