lowing space standards are to serve as guide lines for the design of new buildings or addi tions to existing buildings :1 .Readers' stations at the rate of 25 sq ftper station, with stations to be provided for 25percent of predicted FTE (full-time equivalentstudents) .An additional areaequal to 25 percent of the bound-volume areashould be the budget standard for special mate rials : unbound periodicals, maps, courses ofstudy, and sample textbooks .Book-stack areas at the rate of 0 .10 act ftper volume2 .Special materials .3 .4 .
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