A section of rail track, electrically isolated, forms a circuit controlling a relay.  This relay's state indicates whether the track section is occupied or vacant.
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