The surface prepared to receive the materials for building a railway track, such as ballast, sleepers, and rails, is known as the formation or subgrade. 
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