The prototype uses an NTC thermistor to sense heat.As heat rises, resistance drops, triggering the BJT and turning on the buzzer.Diagram blocks show each component's role.
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