Design: This is a simple, open calorimeter usually made from two Styrofoam cups nested together, with a thermometer and a stirrer.Function: It's primarily used for measuring the heat of reactions occurring in solution, such as neutralization reactions or dissolution processes.It's not sealed, allowing for exchange with the environment.
تم تلخيص النص بواسطة موقع لخصلي © lakhasly.com
