PHYSICAL PROPERTIES OF SILK FIBER :1.Normally, the dry silk fiber has a tenacity varying from 2.4 to 5.1 grams per denier.LusterThe silk fiber's triangular cross-section gives it excellent light reflection.Shape and appearanceSilk filaments are approximately 900 - 1700 meters long.The diameter of the silkfilament is from 9 to 11 microns.Tenacity:Silk fiber is extremely strong.A filament of silk is stronger than an equal diameter filament of steel.2.3.4.
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