Equipment:In some instances, the sealing temperature of the plastic sealing machine exceeded the set parameters, potentially leading to non-conforming sealing quality.
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