Steam Distillation: Steam distillation is employed when the components to be separated are volatile and have high boiling points or when the substances are immiscible with water.
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