Parameters sensitivity to the variation in temperature is considered the main biasing problem intransistor circuits.Besides taking advantage of thehigh output resistance of the current source, it maintains the E I constant.