Set the system as shown in figure (3-1).Find the slope of the straight line you drew in step 8 and use it to , calculate the gravitational acceleration g.Note that the electronically conducting sphere is attached to the release position, which closes the start circuit.Release the sphere from its initial position.From the counter/timer, record the time, t, the sphere takes to reach the pan.