The viscosity of asphalt increased to various degrees with the addition of nanomaterials.The viscosity of nanomaterials in asphalt binder decreased due to the temperature resistance of nanomaterials .The lower mixing and compaction temperatures of nano modified asphalt than the base bitumen can obtain more workability in asphalt.
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