Let's explore the evolution of automatic night light control systems.Theshift to sensor-driven technology marked a significant improvement, with modern devices usingphotodiodes and phototransistors to adjust lighting dynamically based on ambient lightchanges.Originally, these systemsrelied on basic timers to schedule lighting, lacking adaptability to actual lighting conditions.
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