Design: This is a simple, open calorimeter usually made from two Styrofoam cups nested together, with a thermometer and a stirrer.Function: It's primarily used for measuring the heat of reactions occurring in solution, such as neutralization reactions or dissolution processes.It's not sealed, allowing for exchange with the environment.
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