In this year-long study conducted in Cairo, Egypt, an innovative water-based photovoltaic-thermal (PVT) systemcoupled with phase change material (PCM) was evaluated for its ability to enhance building energy efficiency.Economically, the PVT-PCM system achieved a 1.58-year payback period, andcarbon emissions were reduced by 32%, highlighting its viability and environmental benefits.
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