The results can be summarized for the test period without operating the pettier as followso	The maximum productivity of the conventional device is  2100 ml on 8/5/2024 with an amount of 1 cm of water fed into the device, which is equivalent to 8 liters of water.The results for the test period with the peltier running can be summarized as follows o	The maximum productivity of the conventional device is 2260 ml on 27/6/2024 with an amount of 1 cm of water fed into the device, which is equivalent to 8 liters of water.o	The minimum water productivity is 2605 ml on 1/7/ 2024, with 3 cm of water inserted into the device, which is equivalent to 24 liters of water.
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