Greedy routing algorithms demonstrate robust performance in N×N arrays, achieving O(log N) expected packet delay and a maximum queue size of 4 with high probability.  This challenges prior assumptions about their limitations in dynamic environments.  Future research should explore higher-dimensional networks, variable load conditions, hybrid approaches with other optimization techniques, and real-world applications (e.g., IoT, data centers) to improve and validate their effectiveness.
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