Discrete Cosine Transform WatermarkingIn DCT the image is divided into different frequency band, and then embedding watermarkinginto the middle frequency bands of an image.
 DCT represents data in terms of frequency spacerather than an amplitude space. 
DCT based watermarking techniques are robust compared tospatial domain techniques.
Steps in DCT Watermarking Algorithm (Block Based).1.2.3.4.5.6.Divide the image into non-overlapping blocks of 8×8Apply forward DCT to each of these blocksApply some block selection criteria (e.g. HVS)Apply coefficient selection criteriaEmbed watermarkApply inverse DCT transform on each block
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