?A common technique for growing single crystal silicon involves the selective?cooling of molten polycrystalline silicon^2 so that solidification occurs in a?particular crystal direction (Czochralski method).?Typical starting material in a semiconductor fabrication process is a silicon?wafer, which we call now as a substrate.?Crystal growth?
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